



Glasnost: Test if your ISP is shaping your traffic

Detailed test results giving the throughput per flow Glasnost runs:

All BitTorrent and control flow transfers using port 6881

	Transfer Direction
	Bandwidth BitTorrent flow
	Bandwidth control flow

	 

	Download #1
	14736 Kbps
	14679 Kbps

	Download #2
	13782 Kbps
	14590 Kbps

	Download #3
	10029 Kbps
	14416 Kbps

	 

	Upload #1
	197 Kbps
	133 Kbps

	Upload #2
	55 Kbps
	21 Kbps

	Upload #3
	99 Kbps
	89 Kbps


 

All BitTorrent and control flow transfers using port 50816

	Transfer Direction
	Bandwidth BitTorrent flow
	Bandwidth control flow

	 

	Download #1
	12982 Kbps
	14416 Kbps

	Download #2
	6537 Kbps
	11772 Kbps

	Download #3
	12751 Kbps
	14470 Kbps

	 

	Upload #1
	86 Kbps
	179 Kbps

	Upload #2
	32 Kbps
	100 Kbps

	Upload #3
	21 Kbps
	54 Kbps


 

BitTorrent transfers using port 6881 and port 50816

	Transfer Direction
	Bandwidth Port 6881
	Bandwidth Port 50816

	 

	Download #1
	14736 Kbps
	12982 Kbps

	Download #2
	13782 Kbps
	6537 Kbps

	Download #3
	10029 Kbps
	12751 Kbps

	 

	Upload #1
	197 Kbps
	86 Kbps

	Upload #2
	55 Kbps
	32 Kbps

	Upload #3
	99 Kbps
	21 Kbps


 

Control flow transfers using port 6881 and port 50816

	Transfer Direction
	Bandwidth Port 6881
	Bandwidth Port 50816

	 

	Download #1
	14679 Kbps
	14416 Kbps

	Download #2
	14590 Kbps
	11772 Kbps

	Download #3
	14416 Kbps
	14470 Kbps

	 

	Upload #1
	133 Kbps
	179 Kbps

	Upload #2
	21 Kbps
	100 Kbps

	Upload #3
	89 Kbps
	54 Kbps


 

 

For details on our research on broadband networks please refer to our network transparency project webpage
In case you have questions about this tool or our research, please contact us: [image: image1.png]broadband(@mpi-sws.org




